<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">
; B3CC-2.INS - BYE3 insert for CCS-2719 and SDS Z80-SIO - 07/30/85
;
;		  Z80-SIO and 8430 CTC timer
;
; This version is for both the CCS-2719 and Sierra Data Science S-100
; serial I/O boards.  Note:  This is an insert, not an overlay.
;
;    In order to use the CCS-2719 with the Smartmodem,  we must
;    change the hardware somewhat.  The header block on the 2719
;    must be turned over so the port configuration is for DTE
;    (DATA TERMINAL EQUIPMENT).  Further, the standard CCS-2719
;    presents DSR from the DB25 to DCD of the SIO. Bye3 requires
;    the actual DCD from pin 8 of the DB25, Therefore we must
;    remove the jumper in the header block from pins 1 and 15 and add
;    a wire from pin 15 of the flat cable header.  (Pin 8 of the DB25)
;    to pin 1 of the header block.  This will put the modem's DCD signal
;    to the SIO's DCD input. Refer to the CCS-2719 schematic in your user's
;    manual.				- Joe Wright
;
; =   =   =   =   =   =   =   =   =   =   =   =   =   =   =   =   =   =
;
; Select one of the following with YES or NO
;
CCS	EQU	YES		; CCS2719 at 3.6864 MHz for Counter mode
SIERRA	EQU	NO		; Sierra Data Science at 4.000 MHz
;
; Set base port for SIO &amp; CTC chips
;
	 IF	CCS
DPORT	EQU	54H		; Data port
SPORT	EQU	DPORT+1		; Modem satus port
BRPORT	EQU	50H		; Baud rate generator port (CTC)
	 ENDIF			; CCS
;
	 IF	SIERRA
DPORT	EQU	82H		; Data port
SPORT	EQU	DPORT+1		; Modem status port
BRPORT	EQU	89H		; Baud rate generator port (CTC)
	 ENDIF			; SIERRA
;
DAV	EQU	00000001B	; Data available
TBMT	EQU	00000100B	; Transmit buffer empty
DCD	EQU	00001000B	; Data carrier detect
				; [If you have problems, change to 00100000B]
;
; To access CTC baud rate command - Note, the CCS 2719 uses the 3.6864
; MHz xtal for the counter mode and the 4.000 MHz xtal for the timer
; mode.  The SDS board uses the 4.000 MHz master clock for both.
;
; The following assume CCS2719 oscillator at 1.8432 MHz.
;
	 IF	CCS
BD300	EQU	0734H		; 300 baud  (4.000 xtal, rest 1.8432)
BD1200	EQU	4760H		; 1200 baud
BD2400	EQU	4730H		; 2400 baud
	 ENDIF
;
; The following assume	SIERRA DATA SCIENCE oscillator at 4.000 MHz.
;
	 IF	SIERRA
BD300	EQU	0734H		; 300 baud
BD1200	EQU	4768H		; 1200 baud
BD2400	EQU	4734H		; 2400 baud
	 ENDIF
;
;-----------------------------------------------------------------------
;
; See if we still have a carrier - if not, return with the zero flag set
;
MDCARCK:MVI	A,10H		; Reset status
	OUT	SPORT
	IN	SPORT		; Get status
	ANI	DCD		; Check for carrier
	RZ
	ORI	255
	RET
;
; Disconnect and wait for an incoming call
;
MDINIT:	MVI	A,0		; Setup to write register 0
	OUT	SPORT
	MVI	A,18H		; Reset channel
	OUT	SPORT
	MVI	A,4		; Setup to write register 4
	OUT	SPORT
	MVI	A,44H		; Set 16x, 1 stop bit, no parity
	OUT	SPORT
	MVI	A,3		; Setup to write register 3
	OUT	SPORT
	MVI	A,0C1H		; 8 bits, Rx enable
	OUT	SPORT
	MVI	A,5		; Setup to write register 5
	OUT	SPORT
	MVI	A,68H		; DTR off
	OUT	SPORT
;
	PUSH	B		; Save in case it's being used elsewhere
	MVI	B,20		; 2 second delay to drop any carrier
OFFTI:	CALL	DELAY		; 1 second delay
	DCR	B
	JNZ	OFFTI		; Keep looping until finished
	POP	B		; Restore 'BC'
;
	MVI	A,5		; Setup to write register 5
	OUT	SPORT
	MVI	A,0E8H		; Turn DTR back on
	OUT	SPORT
;
	 IF	IMODEM		; If using an intellegent modem
	CALL	IMINIT		; Go initialize it now
	 ENDIF			; IMODEM
;
	RET
;
; Input a character from the modem port
;
MDINP:	IN	DPORT		; Get character
	RET
;
; Check the status to see if a character is available. If not, return
; with the zero flag set.  If yes, use 0FFH to clear the flag.
;
MDINST:	IN	SPORT		; Get status
	ANI	DAV		; Got a character
	RZ			; Return if none
	ORI	255		; Otherwise set the proper flag
	RET
;
; Send a character to the modem
;
MDOUTP:	OUT	DPORT		; Send it
	RET
;
; See if the output is ready for another character
;
MDOUTST:IN	SPORT		; Get status
	ANI	TBMT		; Ready for a character?
	RZ
	ORI	255
	RET
;
; Reinitialize the modem and hang up the phone by dropping DTR and
; leaving it inactive.
;
MDQUIT:	 IF	IMODEM
	CALL	IMQUIT
	 ENDIF			; IMODEM
;
;
; Called by the main program after caller types BYE
;
MDSTOP:	MVI	A,5		; Setup to write register 5
	OUT	SPORT
	MVI	A,68H		; Turn off DTR until next time
	OUT	SPORT
	RET
;
; The following routine sets the baudrate.  BYE3 asks for the maximum
; speed you have available.
;
SET300:	LXI	H,BD300		; Set for 300 baud
	JMP	SETBAUD
;
SET1200:LXI	H,BD1200	; Set for 1200 baud
	JMP	SETBAUD
;
SET2400:LXI	H,BD2400	; Set for 2400 baud
;
SETBAUD:MOV	A,H
	OUT	BRPORT		; Set CTC mode
	MOV	A,L
	OUT	BRPORT		; Set actual speed
	XRA	A		; Say rate is ok
	RET
;			       end
;-----------------------------------------------------------------------
</pre></body></html>