<html><head><meta name="color-scheme" content="light dark"></head><body><pre style="word-wrap: break-word; white-space: pre-wrap;">; B5EA-3.INS  -  Eagle IIE Series insert for BYE5  -  02/15/86
;
;		   Z80 SIO and CTC 8340 timer
;
; Note:  This is an insert, not an overlay.
;
; This version is for the Eagle IIE Series computers using channel 'A'
; Z80 SIO.  The Z80-CTC is used as the baud rate generator.
;
;
; NOTE:  The Eagle does not support DTR on pin 20 or DCD on pin 8, so
;	 be sure you wire the modem cable like this:
;
;		      modem	Eagle
;
;		   TXD	 2  --&gt;  2  RXD
;		   RXD	 3  &lt;--  3  TXD
;		   GND	 7  ---  7  GND
;		   DCD	 8  --&gt;  5  CTS
;		   DTR	20  &lt;--  4  RTS
;
; =   =   =   =   =   =   =   =   =   =   =   =   =   =   =   =   =   =
;
; 02/15/86  Added additional code to poke Baud Rate values to High Memory
;    v3     as the Eagle IIE warm boot routine always looks for a value
;	    in memory and re-initializes the port with these values.
;	    Set the value of HIMEM to your machine.  The three vaules I
;	    have encountered are:
;
;		0DE3AH for bundled hard disk operating system (IIE/IV)
;		0E23AH for Xebec operating system (File 10 added to
;		       floppy system)
;		0EA3AH for floppy-only system  (IIE/II)
;
;	    Also corrected error in the RS-232C Pin-out information for
;	    the Eagle IIE which uses a non-standard convention on the
;	    serial ports.  Pins 2/3 are are reversed from the norm.
;					- Ken Kosakowski
;
; 12/01/85  Fixed the LOADBD routine to output correctly, thanks to
;    v2     Dennis Recla		- Irv Hoff
;
; 07/17/85  Written for use with BYE5	- Irv Hoff
;    v1
; =   =   =   =   =   =   =   =   =   =   =   =   =   =   =   =   =   =
;
;-----------------------------------------------------------------------
;
; Note: For Port A, Data = 18H, CTC = 01H, Port B, Data = 1AH, CTC = 02H
;
PORT	EQU	18H		; Data port
MDCTL1	EQU	PORT+1		; Status/control port
BRPORT	EQU	01H		; Baud rate port
HIMEM	EQU	0E23AH		; Location that the warm boot routine
				; Peeks to re-initialize baudrate on
				; Warm boot
;
BD300	EQU	47D0H		; 62400/300  (first half is CTC command)
BD1200	EQU	4734H		; 62400/1200
BD2400	EQU	471AH		; 62400/2400
;
MBD300	EQU	0734H		; 124800/300  (first half is CTC command)
MBD1200	EQU	4768H		; 124800/1200
MBD2400	EQU	4734H		; 124800/2400
;
;
;-----------------------------------------------------------------------
;
; See if we still have a carrier - if not, return with the zero flag set
;
MDCARCK:MVI	A,10H		; Reset status
	OUT	MDCTL1
	IN	MDCTL1		; Get status
	ANI	20H		; Check for data carrier
	RET
;.....
;
;
; Disconnect and wait for an incoming call
;
MDINIT:	MVI	A,18H		; Reset channel
	OUT	MDCTL1
	MVI	A,4		; Setup to write register 4
	OUT	MDCTL1
	MVI	A,84H		; *1 stop, 8 bits, no parity, 32x
	OUT	MDCTL1
	MVI	A,5		; Setup to write register 5
	OUT	MDCTL1
	MVI	A,68H		; Clear RTS causing hangup
	OUT	MDCTL1
	PUSH	B		; Save in case it's being used elsewhere
	MVI	B,20		; 2 seconds delay to drop any carrier
;
OFFTI:	CALL	DELAY		; 0.1 second delay
	DCR	B
	JNZ	OFFTI		; Keep looping until finished
	POP	B		; Restore bc
	MVI	A,3		; Setup to write register 3
	OUT	MDCTL1
	MVI	A,0C1H		; Initialize receive register
	OUT	MDCTL1
	MVI	A,5		; Setup to write register 5
	OUT	MDCTL1
	MVI	A,0EAH		; Turn on RTS so modem can answer phone
	OUT	MDCTL1
;
	 IF	IMODEM		; If using intelligent modem
	CALL	IMINIT		; Go initialize
	 ENDIF			; IMODEM
;
	RET
;.....
;
;
; Input a character from the modem port
;
MDINP:	IN	PORT		; Get character
	RET
;.....
;
;
; Check the status to see if a character is available.	If not, return
; with the zero flag set.  If yes, use 0FFH to clear the flag.
;
MDINST:	IN	MDCTL1		; Get status
	ANI	01H		; Check receive ready bit
	RZ			; Return if none
	ORI	0FFH		; Otherwise, set the proper flag
	RET
;.....
;
;
; Send a character to the modem
;
MDOUTP:	OUT	PORT		; Send it
	RET
;.....
;
;
; See if the output is ready for another character
;
MDOUTST:IN	MDCTL1
	ANI	04H		; Check transmit ready bit
	RET
;.....
;
;
; Reinitialize the modem and hang up the phone by dropping DTR and
; leaving it inactive.
;
MDQUIT:	 IF	IMODEM		; If using a smartmodem
	CALL	IMQUIT		; Tell it to shut down
	 ENDIF			; IMODEM
;
;
; Called by the main program after caller types BYE
;
MDSTOP:	MVI	A,5		; Setup to write register 5
	OUT	MDCTL1
	MVI	A,68H		; Clear RTS causing shutdown
	OUT	MDCTL1
	RET
;.....
;
;
; The following routine sets the baudrate.  BYE5 asks for the maximum
; speed you have available.
;
SETINV:	ORI	0FFH		; Make sure zero flag is not set
	RET			; Return
;.....
;
;
SET300:	LXI	D,BD300		; Get 300 bps parameters in 'HL' for CTC
	LXI	H,MBD300	; Now get the parameters for high memory
	JMP	LOADBD		; Poke them into memory
;
SET1200:LXI	D,BD1200
	LXI	H,MBD1200
	JMP	LOADBD
;
SET2400:LXI	D,BD2400
	LHLD	MBD2400
;
LOADBD:	MOV	A,D		; CTC command word
	OUT	BRPORT
	MOV	A,E		; Baudrate
	OUT	BRPORT
;
;
; Poke the Eagle CTC code to High Memory
;
	MOV	A,H		; CTC command word
	STA	HIMEM		; Warm boot looks hear for port speed
	MOV	A,L		; Baudrate
	STA	HIMEM+1
	XRA	A		; Show change was satisfactory
	RET
;.....
;
;			       end
;-----------------------------------------------------------------------
</pre></body></html>